|  |  |  |
| --- | --- | --- |
| **Item** | **Designation** | **Coordinates** |
| [A1](file:///E:\\163\\webetm\\webetm\\163\\legend\\l28192000a.html) | Instrument cluster | 15A |
| [A1e53](file:///E:\\163\\webetm\\webetm\\163\\legend\\l28192000a.html) | LOW RANGE indicator lamp | 15B |
| [A55](file:///E:\\163\\webetm\\webetm\\163\\legend\\l28192000a.html) | Transfer case range selection motor | 25D |
| [A55x1](file:///E:\\163\\webetm\\webetm\\163\\legend\\l28192000a.html) | Transfer case range selection motor connector | 24H |
| [F1](file:///E:\\163\\webetm\\webetm\\163\\legend\\l28192000a.html) | Fuse and relay module | 3A 11B |
| [F1f8](file:///E:\\163\\webetm\\webetm\\163\\legend\\l28192000a.html) | Fuse 8 | 10C |
| [F1f22](file:///E:\\163\\webetm\\webetm\\163\\legend\\l28192000a.html) | Fuse 22 | 12C |
| [F1k12](file:///E:\\163\\webetm\\webetm\\163\\legend\\l28192000a.html) | Circuit 15 relay | 6C |
| [G1](file:///E:\\163\\webetm\\webetm\\163\\legend\\l28192000a.html) | Battery | 6H |
| [N10](file:///E:\\163\\webetm\\webetm\\163\\legend\\l28192000a.html) | All-activity module | 2A |
| [N78](file:///E:\\163\\webetm\\webetm\\163\\legend\\l28192000a.html) | Transfer case control module | 9L 16L 23L |
| [S2](file:///E:\\163\\webetm\\webetm\\163\\legend\\l28192000a.html) | Starter switch | 4L |
| [S97/6](file:///E:\\163\\webetm\\webetm\\163\\legend\\l28192000a.html) | Double switch combination | 18H |
| [S97/6e2](file:///E:\\163\\webetm\\webetm\\163\\legend\\l28192000a.html) | Illumination | 18H |
| [S97/6s1](file:///E:\\163\\webetm\\webetm\\163\\legend\\l28192000a.html) | LOW RANGE switch | 19H |
| [W16/4](file:///E:\\163\\webetm\\webetm\\163\\legend\\l28192000a.html) | Ground (output ground - component compartment - right) | 7L |
| [W18](file:///E:\\163\\webetm\\webetm\\163\\legend\\l28192000a.html) | Ground (left front seat crossmember) | 9D |
| [W29/2](file:///E:\\163\\webetm\\webetm\\163\\legend\\l28192000a.html) | Ground (right A-pillar) | 18A |
| [X4/37](file:///E:\\163\\webetm\\webetm\\163\\legend\\l28192000a.html) | Terminal block (circuit 30) | 4F |
| [X12/3](file:///E:\\163\\webetm\\webetm\\163\\legend\\l28192000a.html) | Terminal block (circuit 30, 15, 31, 3-pin) | 5D |
| [X18](file:///E:\\163\\webetm\\webetm\\163\\legend\\l28192000a.html) | Interior and taillamp harness connector, cockpit | 14F 14G 21G 21H |
| [Z50/1](file:///E:\\163\\webetm\\webetm\\163\\legend\\l28192000a.html) | Cockpit connector sleeve (circuit 58d) | 17E |
| [Z50/4](file:///E:\\163\\webetm\\webetm\\163\\legend\\l28192000a.html) | Cockpit connector sleeve (circuit 31, II right) | 17C |
| [Z50/5](file:///E:\\163\\webetm\\webetm\\163\\legend\\l28192000a.html) | Cockpit circuit 30 connector sleeve | 4G |
| [Z50/9](file:///E:\\163\\webetm\\webetm\\163\\legend\\l28192000a.html) | Cockpit connector sleeve (circuit 15 II) | 2G |
| [Z50/11](file:///E:\\163\\webetm\\webetm\\163\\legend\\l28192000a.html) | CAN-L cockpit connector sleeve | 15D |
| [Z50/12](file:///E:\\163\\webetm\\webetm\\163\\legend\\l28192000a.html) | CAN-H cockpit connector sleeve | 14D |
| [Z51/1](file:///E:\\163\\webetm\\webetm\\163\\legend\\l28192000a.html) | Interior connector sleeve (CAN-High 1) | 14H |
| [Z51/2](file:///E:\\163\\webetm\\webetm\\163\\legend\\l28192000a.html) | Interior connector sleeve (CAN-Low 1) | 15H |
| [Z51/5](file:///E:\\163\\webetm\\webetm\\163\\legend\\l28192000a.html) | Interior connector sleeve (circuit 15) | 11G |
| [Z51/9](file:///E:\\163\\webetm\\webetm\\163\\legend\\l28192000a.html) | Interior connector sleeve III (circuit 31, left front seat) | 9G |