|  |  |  |
| --- | --- | --- |
| **Item** | **Designation** | **Coordinates** |
| [A1](file:///E%3A%5C%5C163%5C%5Cwebetm%5C%5Cwebetm%5C%5C163%5C%5Clegend%5C%5Cl28192000b.html)  | Instrument cluster | 16A |
| [A1e53](file:///E%3A%5C%5C163%5C%5Cwebetm%5C%5Cwebetm%5C%5C163%5C%5Clegend%5C%5Cl28192000b.html) | LOW RANGE indicator lamp | 16B |
| [A55](file:///E%3A%5C%5C163%5C%5Cwebetm%5C%5Cwebetm%5C%5C163%5C%5Clegend%5C%5Cl28192000b.html) | Transfer case range selection motor | 27D |
| [A55x1](file:///E%3A%5C%5C163%5C%5Cwebetm%5C%5Cwebetm%5C%5C163%5C%5Clegend%5C%5Cl28192000b.html) | Transfer case range selection motor connector | 25G |
| [F1](file:///E%3A%5C%5C163%5C%5Cwebetm%5C%5Cwebetm%5C%5C163%5C%5Clegend%5C%5Cl28192000b.html)  | Fuse and relay module | 2A10B18K |
| [F1f22](file:///E%3A%5C%5C163%5C%5Cwebetm%5C%5Cwebetm%5C%5C163%5C%5Clegend%5C%5Cl28192000b.html) | Fuse 22 | 11C |
| [F1f8](file:///E%3A%5C%5C163%5C%5Cwebetm%5C%5Cwebetm%5C%5C163%5C%5Clegend%5C%5Cl28192000b.html) | Fuse 8 | 9C |
| [F1k12](file:///E%3A%5C%5C163%5C%5Cwebetm%5C%5Cwebetm%5C%5C163%5C%5Clegend%5C%5Cl28192000b.html) | Circuit 15 relay | 6C |
| [G1](file:///E%3A%5C%5C163%5C%5Cwebetm%5C%5Cwebetm%5C%5C163%5C%5Clegend%5C%5Cl28192000b.html)  | Battery | 5H |
| [N10](file:///E%3A%5C%5C163%5C%5Cwebetm%5C%5Cwebetm%5C%5C163%5C%5Clegend%5C%5Cl28192000b.html)  | All-activity module | 2A |
| [N78](file:///E%3A%5C%5C163%5C%5Cwebetm%5C%5Cwebetm%5C%5C163%5C%5Clegend%5C%5Cl28192000b.html) | Transfer case control module | 8L17L25L |
| [S2](file:///E%3A%5C%5C163%5C%5Cwebetm%5C%5Cwebetm%5C%5C163%5C%5Clegend%5C%5Cl28192000b.html)  | Starter switch | 3L |
| [S97/6](file:///E%3A%5C%5C163%5C%5Cwebetm%5C%5Cwebetm%5C%5C163%5C%5Clegend%5C%5Cl28192000b.html) | Double switch combination | 19G |
| [S97/6e2](file:///E%3A%5C%5C163%5C%5Cwebetm%5C%5Cwebetm%5C%5C163%5C%5Clegend%5C%5Cl28192000b.html) | Illumination | 19G |
| [S97/6s1](file:///E%3A%5C%5C163%5C%5Cwebetm%5C%5Cwebetm%5C%5C163%5C%5Clegend%5C%5Cl28192000b.html) | LOW RANGE switch | 20G |
| [W16/4](file:///E%3A%5C%5C163%5C%5Cwebetm%5C%5Cwebetm%5C%5C163%5C%5Clegend%5C%5Cl28192000b.html)  | Ground (output ground - component compartment - right) | 6L |
| [W18](file:///E%3A%5C%5C163%5C%5Cwebetm%5C%5Cwebetm%5C%5C163%5C%5Clegend%5C%5Cl28192000b.html) | Ground (left front seat crossmember) | 9F |
| [W29/2](file:///E%3A%5C%5C163%5C%5Cwebetm%5C%5Cwebetm%5C%5C163%5C%5Clegend%5C%5Cl28192000b.html) | Ground (right A-pillar) | 19A |
| [X12/12](file:///E%3A%5C%5C163%5C%5Cwebetm%5C%5Cwebetm%5C%5C163%5C%5Clegend%5C%5Cl28192000b.html)  | Circuit 30 terminal block at relay module 1 | 3D |
| [X12/13](file:///E%3A%5C%5C163%5C%5Cwebetm%5C%5Cwebetm%5C%5C163%5C%5Clegend%5C%5Cl28192000b.html) | Circuit 15 terminal block at relay module 1 | 4D |
| [X12/14](file:///E%3A%5C%5C163%5C%5Cwebetm%5C%5Cwebetm%5C%5C163%5C%5Clegend%5C%5Cl28192000b.html) | Circuit 31 terminal block at relay module 1 | 6D |
| [X18](file:///E%3A%5C%5C163%5C%5Cwebetm%5C%5Cwebetm%5C%5C163%5C%5Clegend%5C%5Cl28192000b.html) | Interior and taillamp harness connector, cockpit | 15F23G |
| [X4/37](file:///E%3A%5C%5C163%5C%5Cwebetm%5C%5Cwebetm%5C%5C163%5C%5Clegend%5C%5Cl28192000b.html) | Terminal block (circuit 30) | 4F |
| [Z50/1](file:///E%3A%5C%5C163%5C%5Cwebetm%5C%5Cwebetm%5C%5C163%5C%5Clegend%5C%5Cl28192000b.html)  | Cockpit connector sleeve (circuit 58d) | 18G |
| [Z50/11](file:///E%3A%5C%5C163%5C%5Cwebetm%5C%5Cwebetm%5C%5C163%5C%5Clegend%5C%5Cl28192000b.html) | CAN-L cockpit connector sleeve | 16E |
| [Z50/12](file:///E%3A%5C%5C163%5C%5Cwebetm%5C%5Cwebetm%5C%5C163%5C%5Clegend%5C%5Cl28192000b.html) | CAN-H cockpit connector sleeve | 15E |
| [Z50/4](file:///E%3A%5C%5C163%5C%5Cwebetm%5C%5Cwebetm%5C%5C163%5C%5Clegend%5C%5Cl28192000b.html) | Cockpit connector sleeve (circuit 31, II right) | 19C |
| [Z50/5](file:///E%3A%5C%5C163%5C%5Cwebetm%5C%5Cwebetm%5C%5C163%5C%5Clegend%5C%5Cl28192000b.html) | Cockpit circuit 30 connector sleeve | 4G |
| [Z50/9](file:///E%3A%5C%5C163%5C%5Cwebetm%5C%5Cwebetm%5C%5C163%5C%5Clegend%5C%5Cl28192000b.html) | Cockpit connector sleeve (circuit 15 II) | 2G |
| [Z51/1](file:///E%3A%5C%5C163%5C%5Cwebetm%5C%5Cwebetm%5C%5C163%5C%5Clegend%5C%5Cl28192000b.html) | Interior connector sleeve (CAN-High 1) | 15H |
| [Z51/2](file:///E%3A%5C%5C163%5C%5Cwebetm%5C%5Cwebetm%5C%5C163%5C%5Clegend%5C%5Cl28192000b.html) | Interior connector sleeve (CAN-Low 1) | 16H |
| [Z51/5](file:///E%3A%5C%5C163%5C%5Cwebetm%5C%5Cwebetm%5C%5C163%5C%5Clegend%5C%5Cl28192000b.html) | Interior connector sleeve (circuit 15) | 11H |
| [Z51/9](file:///E%3A%5C%5C163%5C%5Cwebetm%5C%5Cwebetm%5C%5C163%5C%5Clegend%5C%5Cl28192000b.html) | Interior connector sleeve III (circuit 31, left front seat) | 8H |